Cable sizing for LV applications

<http://www.openelectrical.org/wiki/index.php?title=Cable_Sizing_Calculation>

<http://www.cablesizer.com/nec/>

This gives 10AWG (2.56mm dia 5mm2 ) for 4V and 10A

