Sharp IR protection

<https://www.youtube.com/watch?v=ghwU8gVr0yQ>

at 38s of 4mins

47uF, 25v electrolytic capacitor.

47microF 25V capacitor across the supply at the sensor

