Gas inlet strength test

 Ian Crotty

 9 Aug 2016

Temp 24.1degC

See photo of lever arm produced by adding PELD pipe 45mm long plus union

Gas Gaps

CMS RE4-3-TN004

 Corner 01 1.41kg

 Corner 02 2.4 kg

 Corner 03 3.59kg

RE1/2-B005

 Corner 04 1.065kg

 Corner 05 1.45kg