|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  |  | Cooling RE3/1 and RE4/1 | | | |
|  |  |  |  |  |  |  |
|  |  |  |  |  | Ian Crotty 20 March 2017 | |
|  |  |  |  |  |  |  |
| **Power dissipation for PetiRoc with integrated TDC** | | | | | |  |
|  |  |  |  |  |  |  |
| Channel | Chamber | FPGA+GBT | 1 station | 1 YE3 | Rack Power | PetiRoc Dissipation |
|  | 384 | 20 + 1W | 18 |  | Eff 66% |
| [mW] | [watt] | [W] | [W] | [W] | [W] | [W] |
| 6 | 2.304 | 21 | 419 | 839 | 432 | 1271 |
|  |  |  |  |  |  |  |
| One Endcap Power | |  |  |  |  | 1271 |