|  |
| --- |
| **Power dissipation for PetiRoc with integrated TDC** |
|  |  |  |  |  |  |  |
| Channel | Chamber | FPGA+GBT | 1 station | 1 YE3 | Rack Power | PetiRoc Dissipation |
|   | 640 | 20 + 1W | 18 |   | Eff 66% |
| [mW] | [watt] | [W] | [W] | [W] | [W] | [W] |
| 3.6 | 2.304 | 21 | 419 | 839 | 432 | 1271 |
|  |  |  |  |  |  |  |
| One Endcap Power |  |  |  |  | 1271 |