RPC for RE (and RB)

**HV YE1 PP modification from 3-polar to coaxial Jupiter.**

Materials to use

CPE Jupiter chassis male PEEK. 23.100.151-046 (348 F1 Vitone ? Maschio)

Thermo-retractable with glue. Available from Radio spares (RS)

Small dia. 3mm for HV pin. RS 157 3789

Coverage after “Y” dia 9/3mm RS 316 1574

Before “Y” dia. 12/4mm RS 157 3818

Flux (XXXXXXX)

Ian 2 June 2021