Email Christoph about LV cables

Date: Mon, 11 Jun 2018 11:15:15 +0200

From: Christophe Combaret <c.combaret@ipnl.in2p3.fr>

To: Anton Dimitrov <Anton.Dimitrov@cern.ch>,

 Ian Crotty <ian.crotty@cern.ch>,

 Salvatore Buontempo <Salvatore.Buontempo@cern.ch>

Cc: Nicolas Zaganidis <Nicolas.Zaganidis@cern.ch>,

 Laurent Mirabito <laurent.mirabito@cern.ch>,

 "l.mirabito@ipnl.in2p3.fr" <l.mirabito@ipnl.in2p3.fr>,

 Christophe Combaret <Christophe.Combaret@cern.ch>,

 Gabriella Pugliese <gabriella.pugliese@cern.ch>,

 Isabel Pedraza <isapedraza@gmail.com>,

 Imad Laktineh <imad.baptiste.laktineh@cern.ch>

Subject: Re: 1st chamber engineering meeting

Dear collegues,

I also refined cable selction :Â

If we take IS23 rev3 as safety resistance standard (if it is deprecated and

an other one has to be applied, please let us know as soon as possible),

possible materials are :Â

EPR

EPDM

XLPE

Polylefine

Polylefine reticulÃ©

PE cellulaire

PE HD

As commercial materials are not always that clear, I suppose TPE is also

IS23 complient.

That givrs us 3 cables easily available Â :Â

https://fr.rs-online.com/web/p/cable-de-controle-de-commande/8003335/

[fr.rs-online.com]

LAPP KABEL, 0022736 , Â 17AWG , 4 conducteurs , paires torsadees , TPE

https://fr.rs-online.com/web/p/cable-industriel-multiconducteur/7191658/?re

levancy-data=636F3D3126696E3D4931384E525353746F636B4E756D6265724D504E266C75

3D656E266D6D3D6D61746368616C6C26706D3D5E5C647B367D247C5E5C647B377D247C5E5C6

47B31307D2426706F3D313426736E3D592673723D2673743D52535F53544F434B5F4E554D42

45522677633D4E4F4E45267573743D31313233323639267374613D3131323332363926

[fr.rs-online.com]

LAPP KABEL1123269 17AWG LSZH polymere

http://fr.farnell.com/lapp-kabel/281604cy/cable-souple-blinde-4-cond-1-5mm2

/dp/2813528 [fr.farnell.com]

LAPP KABEL 281604CY 4 x 1.5mm2. Â  diam total 9.4mm 16 AWG, polymere

best

C.